零件信息：

**车顶多功能拓展平台安装说明书**

车 型： 坦克300 满顶 （半顶支架减少，横梁减少）

工 时 ： 40 Min

安装前请仔细阅读本安装说明书，以确保正确安装；

为确保可靠性，请严格安装步骤进行安装。

零件构成

请务必在作业前对构成零件进行确认：

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **序号** | **图片** | **产品名称** | **单车用量****(q** | **备注** |
| 1 |   | 车顶平台(Roof Rack) | 1 |  |
| 2 |   | 安装支架(Bracket) | 6 |  |
| 3 |   | 110x30x4.5定制螺丝架(Screw rack) | 6 |  |
| 4 |   | 80x18x4.5双孔垫片(Double hole spacer） | 6 |  |
| 5 |   | 83x21x3 螺帽垫片(Nut spacer) | 6 |  |
| 6 |   | 16x10x6圆柱(Cylinder) | 7 |  |
| 8 |   | 8x40圆柱螺丝(Cylindrical screw) | 12 |  |
| 9 |   | 8x20垫片(Spacer) | 12 |  |
| 10 |   | M8法兰螺帽(Flange nut) | 12 |  |
| 11 |   | 6x20大盘头螺丝 (Large pan head screw) | 20 | 不锈钢 |
| 12 |   | M6-13x20x5方螺母(Square nut) | 15 |  |
| 13 |   | 5x20外六角螺丝(Hexagon Screw) | 10 | 不锈钢 |
| 14 |     | 12mm套筒扳手(Socket wrench) | 1 |  |
| 15 |    | 8mm套筒扳手(Socket wrench) | 1 |  |
| 16 |    | 5mm内六角扳手(Allen wrench) | 1 |  |
| 17 |   | 6mm内六角扳手(Allen wrench) | 1 |  |
| 18 |   |  |  |  |

**安装步骤：**

|  |  |  |
| --- | --- | --- |
| 1 | **安装准备：** ◄ 取出零件确保零件本身完整且整洁。Remove the parts and make sure they are complete and clean.◄ 将组装安好的车顶平台平放在有保护的地面上防止磕伤、划伤。Place the assembled roof platform flat on a protected ground to prevent bumps and scratches （**如需要安装攀梯先安装攀梯**）**Install the ladder firstly if you buy it.**取下原车行李架后塑料盖板，划入110x30x4.5定制螺丝架 \*6个。原车行李框后塑料盖板复原。Remove the rear plastic cover of the original roof rack and insert 6 screw racks of 110x30x4.5. Restorae original rear plastic cover of roof rack.注意后1定制螺丝架与 原车行李框后塑料盖板之间留6公分距离。如图。(左右相同)**Note**: There is a 6 cm distance between the rear screw bracket and the rear plastic cover of the original car roof rack. As shown in the picture. (Same as left and right) |    |
| 2 | **安装支架与车顶平台本体连接：**取出安装支架，与提前安装好的定制螺丝架,预安装不要紧固，使用M8法兰螺帽\*2，如图安装，一边3个。**注意：此处为预固定。**Take out the installation bracket and pre-install it with the pre-installed screw bracketm but not tighten. Use M8 flange nuts\*2, as shown in the figure to install, 3 on each side.**Note: This is pre-fixed.** |
| 3 | **车顶平台整体放到车顶上：**需2-3人将平台置于车顶，调整前后距离，以后1安装支架为基准点。调整其余2个安装支架与平台孔位对准。It takes 2-3 people to place the roof rack on the car roof, adjust the front and rear distance, and use the rear 1 mounting bracket as the reference point. Adjust the remaining 2 mounting brackets to align with the platform holes.**安装支架与车顶平台本体连接：**安装支架与平台，使用M8\*40圆柱内六角螺栓\*2+M8垫片\*2+双孔垫片\*1+双孔带螺母垫片\*1，如图安装支架与车顶平台本体连接（共6个支架）全部预安装后紧固所有螺丝。To install the bracket and roof rack, use M8\*40 cylindrical hexagon socket bolts\*2+M8Spacer\*2+double-hole Spacer\*1+double-hole nut sapcer\*1, as shown in the figureThe mounting brackets are connected to the roof rack body (a total of 6 brackets) and all are pre-installed before tightening all screws. |    |
|  | **安装完成总装图****Installation completed diagram** |   |